DVB PARSER

Main:

Buffer of TS file Size

Transport stream file

PID filter buffers of size 4K is initialized for all registered PID’s

PID FILTERING:

TS Buffer